{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Plan1","Plan2","Plan3"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Plan1","index":0,"n_rows":16,"n_cols":12,"rows_kept":16,"cut":false,"hidden":false,"merged":[[1,0,2,11],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[9,0,9,2]],"flags":["formulas_cached_only"]}
[]
["VAZÃO EM UM ORIFICIO PARA DIFERENTES CARGAS HIDRAÚLICAS"]
[]
["Tempo(s)",0,1,2,3,4,5,6,7,8,9,10]
["Altura Hidraulica(m)",0,0.2,0.4,0.6,0.8,1,1.5,2,3,5,10]
["Cd (variável com H e D)",0,0.653,0.651,0.648,0.645,0.642,0.638,0.636,0.634,0.634,0.634]
["Vazão (L/s)",0,0.4061683582064378,0.5726495088963476,0.6981175235537058,0.802384658631401,0.8929207933297536,1.086786454013889,1.2509790073037323,1.5273121041577693,1.9717514479546827,2.7884776393263]
["Incremento de vazão (L/s):",2.3823092811198623]
[]
["Orifício Vertical"]
["Tipo","Circular de parede fina"]
["Diâmetro (m)",0.02]
["Área do orifício(m2)",0.0003141592653589793]
["Cof. De descarga (Cd)","variável com H e D"]
[]
["Células em amarelho precisam ser modificadas"]

{"sheet":"Plan2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Plan3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}