{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["PLANIMETRIA"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PLANIMETRIA","index":0,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[[4,0,4,8],[0,0,0,8],[1,0,1,8],[3,0,3,8],[34,0,34,9],[8,2,8,3],[8,0,8,1],[11,0,11,1],[30,1,30,2],[30,3,30,4],[11,2,11,3],[20,5,20,8],[30,5,30,8],[22,7,22,8],[12,7,13,7],[12,3,13,4],[14,3,14,4],[19,0,19,1],[12,0,13,0],[12,1,13,1],[12,5,13,5],[12,6,13,6],[16,3,16,4],[12,8,13,8],[19,3,19,4],[11,5,11,6],[22,0,23,0],[22,1,22,2],[22,3,22,4],[22,5,22,6],[12,2,13,2],[15,3,15,4],[9,5,9,6],[10,5,10,6],[6,6,6,8],[7,6,7,8],[10,2,10,3],[2,0,2,9],[5,0,5,8],[10,0,10,1],[6,1,6,4],[7,1,7,4],[9,0,9,1],[9,2,9,3],[20,0,20,1],[20,3,20,4],[17,3,17,4],[18,3,18,4]],"flags":["formulas_cached_only"]}
["UNIVERSIDADE REGIONAL DO CARIRI - URCA"]
["CENTRO DE CIÊNCIA E TECNOLOGIA -CCT"]
["DEPARTAMENTO DE CONSTRUÇÃO CIVIL"]
["Disciplina: Topografia III"]
["Professor: Renato de Oliveira Fernandes"]
["PLANILHA PARA CÁLCULO DE POLIGONAL FECHADA"]
["Cliente:",{"$nulls":4},"Data:"]
["Local:",{"$nulls":4},"Responsável:"]
["Resolução do Aparelho:",null,5.7870370370370366e-05]
["Azim. inicial (1-2):",null,7.760416666666667,null,null,"Coordenadas de Origem:",null,"Valor","Vértice"]
["Tolerância Angular (2*Resol.*(N)0,5):",null,0.00025880416406247564,null,null,"X mais ao Oeste (m):",null,0,5]
["Tolerância Linear (ex. 1/1000):",null,0.001,null,null,"Y mais ao Sul (m):",null,0,3]
["ESTAÇÃO","Ponto Visado","Distância (d)","Ângulo (Ain)",null,"Correção Angular (Cn)","Ângulo Corrigido (Ainc)","Az ré","Azimute (Azn)"]
[{"$nulls":9},"Contorno"]
[1,2,57.76,1.530787037037037,null,3.472222222242749e-05,1.5308217592592592,"-",7.760416666666667,7.5]
[2,3,53.39,8.994386574074074,null,3.472222222242749e-05,8.994421296296297,0.26041666666666696,6.265995370370369,15]
[3,4,60.28,2.1530671296296298,null,3.472222222242749e-05,2.153101851851852,13.76599537037037,11.612893518518517,0]
[4,5,43.39,4.629513888888889,null,3.472222222242749e-05,4.629548611111112,4.112893518518517,14.483344907407405]
[5,1,71.49,5.192071759259259,null,3.472222222242749e-05,5.192106481481482,6.983344907407405,1.7912384259259229]
["SOMA (å)",null,286.31,22.499826388888888,null,0.00017361111111213745,22.5]
["Erro angular (e)",null,0.00017361111111213745,"Verif. do erro ang.:",null,"Compensar Erro"]
[]
["ESTAÇÃO","Projeções",null,"Correções",null,"Projeções Corrigidas",null,"Coordenandas Topográficas"]
[null,"Dx","Dy","Cx","Cy","Dxc","Dyc","X","Y"]
[1,-6.288150691449484,-57.41669409572118,0.0118878674576865,0.006598976131312155,-6.2762628239917975,-57.41009511958987,48.76139683739535,103.8189123902659]
[2,26.384608800182267,-46.41491698216581,0.010988456432927325,0.0060997114897984065,26.395597256615194,-46.40881727067602,42.48513401340355,46.408817270676025]
[3,-59.58490770636038,9.127824145135312,0.01240652095480163,0.006886881599645026,-59.57250118540558,9.134711026734957,68.88073127001874,0]
[4,-9.317160392248018,42.37785532828584,0.008930307634851406,0.004957229472604474,-9.308230084613166,42.38281255775844,9.308230084613164,9.134711026734957]
[5,48.74668313163791,52.29322120183158,0.014713705757444734,0.008167603940919425,48.76139683739535,52.3013888057725,0,51.5175235844934]
["SOMA",-0.0589268582377116,-0.03271040263427949,0.05892685823771159,0.03271040263427949,0,0,"Área (m2):",3373.899397262544]
["Precisão:",0.00023539842044144777,null,"Verif. do erro linear:",null,"Compesar Erro"]
[]
["Observação: todos os dados destacado em vermelho deve ser preenchido pelo usuário."]
[]
["CROQUI DA POLIGONAL"]